|  |  |
| --- | --- |
| Product Name | 10mm micro stepper motor |
| Rated Voltage | 5.0 V DC |
| Current Per Phase | 50mA /phase |
| Coil Resistance | 55Ω±10% |
| No. Of phase | 2 Phases |
| Step Angle | 18 degree |
| Max. Starting Frequency | 1000 PPS min (AT 5.0 V DC) |
| Max. Slewing Frequency | 1800 PPS min (AT 5.0 V DC) |
| Pull-In Torque | 2.0 gf.cm min(AT 500 PPS 5.0 V DC) |
| Pull-Out Torque | 2.2 gf.cm min(AT 500 PPS 5.0 V DC) |